}

# lum_rm_stat_strip_te_c (RM)

Foundry strip ring modulator - C band TE

## Keywords

## Ports

Name | Type
--- | ---
ele_cat | Electrical Signal
ele_an | Electrical Signal
ele_th_1 | Electrical Signal
ele_th_2 | Electrical Signal
opt_1 | Optical Signal
opt_2 | Optical Signal

## Properties

### General Properties

Name | Default value | Default unit | Range
--- | --- | --- | ---
name | lum_rm_stat_strip_te_c | - | -
enabled | true | - | [true, false]
description | Foundry strip ring modulator - C band TE | - | -
prefix | RM | - | -
model | lum_rm_stat_strip_te_c | - | -
library | - | - | -

### Thermal Properties

Name | Default value | Default unit | Range
--- | --- | --- | ---
temperature | %temperature% | K | (-∞, +∞)

### Design Kit Properties

Name | Default value | Default unit | Range
--- | --- | --- | ---
internal electrical equivalent | %internal electrical equivalent% | - | [true, false]

### CML/Notes Properties

Name | Default value | Default unit | Range
--- | --- | --- | ---
wavelength_range | C-band (1530 - 1565 nm) | - | -
bias_range_phase_shifter | [-2 V, 0.5 V] | - | -
bias_range_thermal_tuner | [0 V, 5 V] | - | -
polarization | TE | - | -
time_domain_requirement | minimum sample rate = 5.5 THz (time domain simulations only) | - | -

### CML Properties

Name | Default value | Default unit | Range
--- | --- | --- | ---
internal delay compensation | false | - | [true, false]
delay compensation | 0 | - | [0, 100]

### CML/Statistical Properties

Name | Default value | Default unit | Range
--- | --- | --- | ---
delta_height | 0 | - | (-∞, +∞)
delta_width | 0 | - | (-∞, +∞)
delta_ridge_height | 0 | - | (-∞, +∞)