}

# lum_mzm_stat_unbalanced_te_c (MZM)

Foundry MZM - C band TE

## Keywords

## Ports

Name | Type
--- | ---
opt_1 | Optical Signal
opt_2 | Optical Signal
ele_h1+ | Electrical Signal
ele_h1- | Electrical Signal
ele_h2+ | Electrical Signal
ele_h2- | Electrical Signal
ele_an_top | Electrical Signal
ele_cat_top | Electrical Signal
ele_an_bottom | Electrical Signal
ele_cat_bottom | Electrical Signal

## Properties

### General Properties

Name | Default value | Default unit | Range
--- | --- | --- | ---
name | lum_mzm_stat_unbalanced_te_c | - | -
enabled | true | - | [true, false]
description | Foundry MZM - C band TE | - | -
prefix | MZM | - | -
model | lum_mzm_stat_unbalanced_te_c | - | -
library | - | - | -

### Thermal Properties

Name | Default value | Default unit | Range
--- | --- | --- | ---
temperature | %temperature% | K | (-∞, +∞)

### Design Kit Properties

Name | Default value | Default unit | Range
--- | --- | --- | ---
internal electrical equivalent | %internal electrical equivalent% | - | [true, false]

### CML/notes Properties

Name | Default value | Default unit | Range
--- | --- | --- | ---
wavelength_range | C-band (1530 - 1570 nm) | - | -
bias_range_phase_shifter | [-4 V, 0.5 V] | - | -
bias_range_thermal_tuner | [0 V, 5 V] | - | -

### CML Properties

Name | Default value | Default unit | Range
--- | --- | --- | ---
internal delay compensation | false | - | [true, false]
delay compensation | 0 | - | [0, 100]

### CML/Statistical Properties

Name | Default value | Default unit | Range
--- | --- | --- | ---
delta_height_upper | 0 | - | (-∞, +∞)
delta_height_lower | 0 | - | (-∞, +∞)
delta_width_upper | 0 | - | (-∞, +∞)
delta_width_lower | 0 | - | (-∞, +∞)
delta_ridge_height_upper | 0 | - | (-∞, +∞)
delta_ridge_height_lower | 0 | - | (-∞, +∞)