}

# lum_mmi_stat_1x2_strip_te_c (MMI)

Foundry fixed strip 1x2 multimode interference coupler with statistical variations enabled - C band TE

## Keywords

## Ports

Name | Type
--- | ---
opt_1 | Optical Signal
opt_2 | Optical Signal
opt_3 | Optical Signal

## Properties

### General Properties

Name | Default value | Default unit | Range
--- | --- | --- | ---
name | lum_mmi_stat_1x2_strip_te_c | - | -
enabled | true | - | [true, false]
description | Foundry fixed strip 1x2 multimode interference coupler with statistical variations enabled - C band TE | - | -
prefix | MMI | - | -
model | lum_mmi_stat_1x2_strip_te_c | - | -
library | - | - | -

### CML/Notes Properties

Name | Default value | Default unit | Range
--- | --- | --- | ---
Pcell | This is a parameterized model based on S-parameters. | - | -
wavelength_range | C-band (1530 - 1565 nm) | - | -
polarization | TE | - | -

### CML Properties

Name | Default value | Default unit | Range
--- | --- | --- | ---
delay compensation | 0 | - | [0, 100]

### CML/Statistical Properties

Name | Default value | Default unit | Range
--- | --- | --- | ---
delta_height | 0 | - | (-∞, +∞)
delta_width | 0 | - | (-∞, +∞)