}

# lum_ps_thermal_te_c (PSTH)

Foundry thermal phase shifter - C band TE

## Keywords

## Ports

Name | Type
--- | ---
opt_1 | Optical Signal
opt_2 | Optical Signal
ele_h1 | Electrical Signal
ele_g1 | Electrical Signal

## Properties

### General Properties

Name | Default value | Default unit | Range
--- | --- | --- | ---
name Defines the name of the element. | lum_ps_thermal_te_c | - | -
enabled Defines whether or not the element is enabled. | true | - | [true, false]
description A brief description of the elements functionality. | Foundry thermal phase shifter - C band TE | - | -
prefix Defines the element name prefix. | PSTH | - | -
model Defines the element model name. | lum_ps_thermal_te_c | - | -
library Defines the element location or source in the library (custom or design kit). | ::Custom::lumfoundry_template::Phase Shifters | - | -

### Thermal Properties

Name | Default value | Default unit | Range
--- | --- | --- | ---
temperature Defines the temperature. | %temperature% | K | (-∞, +∞)

### Design Kit Properties

Name | Default value | Default unit | Range
--- | --- | --- | ---
version | 4.0 | - | -

### CML Properties

Name | Default value | Default unit | Range
--- | --- | --- | ---
enable_thermal_time_constant | false | - | [true, false]
internal delay compensation | false | - | [true, false]
delay compensation | 0 | - | [0, 100]

### CML/Notes Properties

Name | Default value | Default unit | Range
--- | --- | --- | ---
wavelength_range | C-band (1530 - 1565 nm) | - | -
bias_range | [0 V, 10 V] | - | -

## Results

Name | Description
--- | ---
diagnostic/response #/transmission | The complex transmission vs. frequency corresponding to the ideal and designed filter.
diagnostic/response #/gain | The gain vs. frequency corresponding to the ideal and designed filter.
diagnostic/response #/error | Mean square error comparing the frequency response of the designed filter implementation with the ideal frequency response.