###### - Version:

Ansys Zemax OpticStudio – 26R1.02
Ansys Discovery – 26R1

###### - Notes:

IMPORTANT: This is an illustrative example for the import of CFD Data into Ansys Zemax OpticStudio (SOFT Analysis) – This is not a realistic Yb:YAG Laser amplifier system and simplification and assumption have been made.

If you are interested in receiving further information, example files and a live demo on the Ansys optiSLang part of this workflow, please reach out to your Ansys, Part of Synopsys, representative.

For Direct Index import into Ansys Zemax OpticStudio: Region A = Surface 6 (Z Transformation -13.85); Region B = Surface 10 ( No Z Transformation); Region C = Surface 14 (Z Transformation +13.84). Transformation are necessary due to a flipped coordinate system in Discovery.

By Flurin Herren,
